|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  | | --- | |  | | http://www.nitgen.com/eng/product/img/tit_hamster3.jpg | |  | | |  |  |  |  |  | | --- | --- | --- | --- | --- | | http://www.nitgen.com/eng/product/img/Hamster3.jpg | |  | | --- | | FINGKEY Hamster Ⅲ has a fingerprint sensing function and is a cutting-edge fingerprint sensor that prevents use of fake fingerprints. It can be connected to PC along with a nomal mouse and used for all the areas involving passwords and will be a competent security gadget without having to use a password, which is often hard to remember and misused by unauthorized persons. | |  | |  | | | |  | | |  |  |  | | --- | --- | --- | | [http://www.nitgen.com/eng/product/img/tab01.jpg](http://www.nitgen.com/eng/product/Hamster3.html#a1) | [http://www.nitgen.com/eng/product/img/tab02.jpg](http://www.nitgen.com/eng/product/Hamster3.html#a2) | [http://www.nitgen.com/eng/product/img/tab_enbioscan_03.jpg](http://www.nitgen.com/eng/product/Hamster3.html#a3) | | | http://www.nitgen.com/eng/product/img/stit01.jpg | | |  | | --- | | http://www.nitgen.com/eng/product/img/box_top.jpg | | http://www.nitgen.com/eng/product/img/icon.jpg Ergonomic Design    - Change to two type model http://www.nitgen.com/eng/product/img/icon.jpg USB Connection    - USB 2.0 compatible interface, plug and play device    - Supports multiple devices handling http://www.nitgen.com/eng/product/img/icon.jpg Superior Matching Engine    - 1st in FVC(Fingerprint Verification Competition)    - Auto-on™ Function  http://www.nitgen.com/eng/product/img/icon.jpg Advanced Optical Technology    - Sensor resistant to scratches, impact, vibration and electrostatic shock http://www.nitgen.com/eng/product/img/icon.jpg International Standard Image Format and Interfaces    - WSQ compression    - ISO 19794-2/4, ANSI 378, NFIQ http://www.nitgen.com/eng/product/img/icon.jpg High Quality Image Capturing http://www.nitgen.com/eng/product/img/icon.jpg Strong Performance for Wet / Dry Finger | | http://www.nitgen.com/eng/product/img/box_bot.jpg | | | http://www.nitgen.com/eng/product/img/stit02.jpg | | |  |  |  | | --- | --- | --- | |  | | | | http://www.nitgen.com/eng/product/img/nac5000_t01.jpg | http://www.nitgen.com/eng/product/img/t_bar.jpg | http://www.nitgen.com/eng/product/img/t_03.jpg | |  | | |  |  |  | | --- | --- | | Optical Sensor | OPP06 | |  | | | Size (mm) | 68 x 68 x 81 (With Stand)   30 x 48.5 x 70 (Without Stand) | |  | | | Image Size | 248 x 292 pixels | |  | | | Resolution | 500 DPI | |  | | | Interface | USB 2.0 High/Full Speed | |  | | | Image acquisition time | Full Speed : Avg. 500 msec.   High Speed : Avg. 300 msec. | |  | | | Operating Temperature | -20~60 ℃ | |  | | | Operating Humidity | < RH 90% | |  | | | Power Source | USB BUS Power | |  | | | OS | Windows2000 or higher, Windows Server 2003/2008, Linux Kernel 2.6.x | |  | | | Certificated | KC, UL, CE, FCC | |  | | | |  | | http://www.nitgen.com/eng/product/img/stit06.jpg | | |  | | --- | | http://www.nitgen.com/eng/product/img/box_top.jpg | | http://www.nitgen.com/eng/product/img/icon.jpg Computer security  http://www.nitgen.com/eng/product/img/icon.jpg IT solution(Groupware, etc.)  http://www.nitgen.com/eng/product/img/icon.jpg e-commerce http://www.nitgen.com/eng/product/img/icon.jpg Security for bank and financial system http://www.nitgen.com/eng/product/img/icon.jpg Health care system http://www.nitgen.com/eng/product/img/icon.jpg Substitution for password | | |